<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="6.4">
<drawing>
<board>
<plain>
<wire x1="0" y1="16.373" x2="0" y2="0.635" width="0" layer="20"/>
<wire x1="0" y1="0.635" x2="0.635" y2="0" width="0" layer="20" curve="90"/>
<wire x1="0.635" y1="0" x2="18.466" y2="0" width="0" layer="20"/>
<wire x1="18.466" y1="0" x2="19.101" y2="0.635" width="0" layer="20" curve="90"/>
<wire x1="19.101" y1="0.635" x2="19.101" y2="16.373" width="0" layer="20"/>
<wire x1="19.101" y1="16.373" x2="18.466" y2="17.008" width="0" layer="20" curve="90"/>
<wire x1="18.466" y1="17.008" x2="0.635" y2="17.008" width="0" layer="20"/>
<wire x1="0.635" y1="17.008" x2="0" y2="16.373" width="0" layer="20" curve="90"/>
<text>TOC2WD 2013</text>
<text>Alan Smith</text>
<text>0</text>
<text>1</text>
<text>2</text>
<text>3</text>
<text>GND</text>
<text>VCC</text>
<text>MOSI</text>
<text>!RST</text>
<text>SCK</text>
<text>MISO</text>
</plain>
<libraries>
<library name="SparkFun-DigitalIC">
<description>&lt;h3&gt;SparkFun Electronics' preferred foot prints&lt;/h3&gt;
In this library you'll find all manner of digital ICs- microcontrollers, memory chips, logic chips, FPGAs, etc.&lt;br&gt;&lt;br&gt;
We've spent an enormous amount of time creating and checking these footprints and parts, but it is the end user's responsibility to ensure correctness and suitablity for a given componet or application. If you enjoy using this library, please buy one of our products at www.sparkfun.com.
&lt;br&gt;&lt;br&gt;
&lt;b&gt;Licensing:&lt;/b&gt; CC v3.0 Share-Alike You are welcome to use this library for commercial purposes. For attribution, we ask that when you begin to sell your device using our footprint, you email us with a link to the product being sold. We want bragging rights that we helped (in a very small part) to create your 8th world wonder. We would like the opportunity to feature your device on our homepage.</description>
<packages>
<package name="SO08-EIAJ">
<description>Fits EIAJ packages (wide version of the SOIC-8).</description>
</package>
</packages>
</library>
<library name="adafruit">
<packages>
<package name="CHIPLED_1206">
<description>&lt;b&gt;CHIPLED&lt;/b&gt;&lt;p&gt;
Source: http://www.osram.convergy.de/ ... LG_LY N971.pdf</description>
</package>
</packages>
</library>
<library name="dp_devices">
<description>Dangerous Prototypes Standard PCB sizes
http://dangerousprototypes.com</description>
<packages>
<package name="RN8P-4R-CRA06S">
</package>
</packages>
</library>
<library name="caudle">
<packages>
<package name="2X5_EDGE">
</package>
</packages>
</library>
<library name="switch-tact">
<description>&lt;b&gt;Diptronics THMD &amp; SMD tact switches&lt;/b&gt;
&lt;p&gt;&lt;ul&gt;
&lt;li&gt;DTS-3: 3.5x6mm THMD tact switch
&lt;li&gt;DTS-6, DTS-64: 6x6mm THMD tact switch
&lt;li&gt;DTSM-3: 3.5x6mm SMD tact switch
&lt;li&gt;DTSM-6, DTSM-64: 6x6mm SMD tact switch
&lt;/ul&gt;&lt;/p&gt;
&lt;p&gt;&lt;b&gt;Doublecheck before using!&lt;/b&gt;&lt;/p&gt;</description>
<packages>
<package name="DTSM-6">
</package>
</packages>
</library>
</libraries>
<attributes>
</attributes>
<variantdefs>
</variantdefs>
<elements>
<element name="U1" library="SparkFun-DigitalIC" package="SO08-EIAJ" value="Tiny85-20-SMT">
<attribute name="PROD_ID" value="IC-09092"/>
</element>
<element name="LED1" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED2" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED3" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="VALUE"/>
</element>
<element name="LED4" library="adafruit" package="CHIPLED_1206" value="">
<attribute name="VALUE"/>
</element>
<element name="RN1" library="dp_devices" package="RN8P-4R-CRA06S" value="">
<attribute name="VALUE"/>
</element>
<element name="U$2" library="caudle" package="2X5_EDGE" value="2X5_EDGE"/>
<element name="S2" library="switch-tact" package="DTSM-6" value="DTSM-6"/>
</elements>
<signals>
<signal name="GND">
<contactref element="U1" pad="4"/>
<contactref element="S2" pad="3"/>
<contactref element="RN1" pad="5"/>
<contactref element="RN1" pad="6"/>
<contactref element="RN1" pad="7"/>
<contactref element="RN1" pad="8"/>
<contactref element="U$2" pad="4_GND"/>
<contactref element="U$2" pad="6_GND"/>
<contactref element="U$2" pad="8_GND"/>
<contactref element="U$2" pad="10_GND"/>
</signal>
<signal name="MOSI">
<contactref element="U1" pad="5"/>
<contactref element="LED1" pad="A"/>
<contactref element="U$2" pad="1_MOSI"/>
</signal>
<signal name="MISO">
<contactref element="U1" pad="6"/>
<contactref element="LED2" pad="A"/>
<contactref element="U$2" pad="9_MISO"/>
</signal>
<signal name="SCK">
<contactref element="U1" pad="7"/>
<contactref element="LED3" pad="A"/>
<contactref element="U$2" pad="7_SCK"/>
</signal>
<signal name="!RST">
<contactref element="U1" pad="1"/>
<contactref element="U$2" pad="5_!RST"/>
</signal>
<signal name="N$13">
<contactref element="LED4" pad="A"/>
<contactref element="U1" pad="2"/>
</signal>
<signal name="N$14">
<contactref element="U1" pad="3"/>
<contactref element="S2" pad="1"/>
</signal>
<signal name="N$1">
<contactref element="LED2" pad="C"/>
<contactref element="RN1" pad="3"/>
</signal>
<signal name="N$2">
<contactref element="LED1" pad="C"/>
<contactref element="RN1" pad="4"/>
</signal>
<signal name="N$3">
<contactref element="LED3" pad="C"/>
<contactref element="RN1" pad="2"/>
</signal>
<signal name="N$4">
<contactref element="LED4" pad="C"/>
<contactref element="RN1" pad="1"/>
</signal>
<signal name="VCC">
<contactref element="U$2" pad="2_VCC"/>
<contactref element="U1" pad="8"/>
</signal>
</signals>
</board>
</drawing>
</eagle>
